IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "dv570.ifc"
Time stamp: "2020-11-25T12:22:37"
Preprocessor: "SwIFC"
Application: by Organization id "SW"

People and organizations
  Person (no name given) of Organization (no name given)
  Owner history of Person (no name given) of Organization (no name given) | application by Organization id "SW" | change ADDED | created 1417173800 (2014-11-28T11:23:20Z) | last modified 1417173800 (2014-11-28T11:23:20Z) by Person (no name given) of Organization (no name given) with by Organization id "SW"

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  POWERUNIT: KILO WATT
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  MASSUNIT: KILO GRAM
  ELECTRICVOLTAGEUNIT: VOLT
  ELECTRICCURRENTUNIT: AMPERE
  TIMEUNIT: SECOND
  VOLUMETRICFLOWRATEUNIT: derived
  LINEARVELOCITYUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 0° 0′ 0″ | longitude 0° 0′ 0″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "Default Building Storey" | long name "Default Building Storey" | elevation 0.
        contains 1 element
          1 x IFCENERGYCONVERSIONDEVICE | type IFCUNITARYEQUIPMENTTYPE "Family1" | object type "AHU 1" | names: "Pos 1/0" | property sets: Identity Data, Dimensions, Mechanical, Mechanical - Flow, Electrical - Circuiting

Types
  IFCUNITARYEQUIPMENTTYPE "Family1" | AIRCONDITIONINGUNIT | 1 occurrence

Property sets
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Device_adu_id = "11" (IFCLABEL)
    Device_design_version = "13" (IFCLABEL)
    Device_dutypoint_version = "2" (IFCLABEL)
    Position = "AHU 1" (IFCLABEL)
    Project_date = "21.2.2019" (IFCLABEL)
    Project_name = "" (IFCLABEL)
    Source_adu_file = "C:\Users\dgavril\Desktop\atrea.adu" (IFCLABEL)
    Type = "DUPLEXVENT 570 EC5.RD5" (IFCLABEL)
  Dimensions | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Height = 0.930 (IFCLENGTHMEASURE) [METRE]
    Length = 1.290 (IFCLENGTHMEASURE) [METRE]
    Weight = 72 (IFCMASSMEASURE) [KILO GRAM]
    Width = 0.370 (IFCLENGTHMEASURE) [METRE]
  Mechanical | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Casing_mat = "painted zinc layer" (IFCLABEL)
    Inner_surface = "Pozink" (IFCLABEL)
    Installation_environment = "" (IFCLABEL)
    Insulation_thickness = 0.050 (IFCLENGTHMEASURE) [METRE]
    Insulation_type = "PUR" (IFCLABEL)
    Outer_surface = "RAL 9002" (IFCLABEL)
    Panel_thickness = 0.060 (IFCLENGTHMEASURE) [METRE]
    Recuperation_type = "Plate heat recovery exchanger" (IFCLABEL)
  Mechanical - Flow | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Exhaust_SFP = 0.000 (IFCREAL)
    Exhaust_air_speed = 0.000 (IFCLINEARVELOCITYMEASURE) [derived]
    Exhaust_airflow = 0.000 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Exhaust_ext_pressure = 0 (IFCPRESSUREMEASURE)
    Exhaust_inlet_hum = 40.0 (IFCREAL)
    Exhaust_inlet_temp = 20.0 (IFCTHERMODYNAMICTEMPERATUREMEASURE) [DEGREE_CELSIUS]
    Exhaust_outlet_hum = 0.0 (IFCREAL)
    Exhaust_outlet_temp = 0.0 (IFCTHERMODYNAMICTEMPERATUREMEASURE) [DEGREE_CELSIUS]
    Recuperation_efficiency_EN308 = 0.00 (IFCREAL)
    Supply_SFP = 0.000 (IFCREAL)
    Supply_air_speed = 0.000 (IFCLINEARVELOCITYMEASURE) [derived]
    Supply_airflow = 0.000 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Supply_ext_pressure = 0 (IFCPRESSUREMEASURE)
    Supply_inlet_hum = 90.0 (IFCREAL)
    Supply_inlet_temp = -5.0 (IFCTHERMODYNAMICTEMPERATUREMEASURE) [DEGREE_CELSIUS]
    Supply_outlet_hum = 90.0 (IFCREAL)
    Supply_outlet_temp = -5.0 (IFCTHERMODYNAMICTEMPERATUREMEASURE) [DEGREE_CELSIUS]
    Total_SFP = 0.000 (IFCREAL)
  Electrical - Circuiting | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Current_max = 2.80 (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Input_power_max = 0.34 (IFCPOWERMEASURE) [KILO WATT]
    Phases_count = 1 (IFCINTEGER)
    Power_supply_cable = "0" (IFCLABEL)
    Power_supply_fusing = "0" (IFCLABEL)
    Voltage = 230 (IFCELECTRICVOLTAGEMEASURE) [VOLT]